EMD GP38-2

| Technical Data Total Built: 2213 Length: 59' 2" (18.03m) Engine Power: 2,000Hp (1.49MW)

The EMD GP38-2 is a four-axle diesel-electric road switcher type locomotive built by General Motors, Electro-Motive Division. Part of the EMD Dash 2 line, the GP38-2 was an upgraded version of the earlier GP38. Power is provided by an EMD 645E 16-cylinder engine, which generates 2000 horsepower (1.5 MW). Most units remain in service.

The GP38-2 differs externally from the earlier GP38 only in minor details. Its most distinctive identifying feature is the cooling water level sight glass on the right side of the long hood. The battery box covers of the Dash 2s are bolted down instead of hinged. The GP38-2 is available with either a high-short-hood, common on Norfolk Southern units, or a low-short-hood, which is found on most other railroads.

A total of 2213 units were built. 1,799 examples were built for American railroads and industrial concerns, 257 for Canadian railroads and industrials, 156 for Mexican railroads and industrials, and 1 export unit for the Saudi Government Railways.