GE C40-8W

| Technical Data Total Built: 756t Length: 70'8" (21.54m) Engine Power: 4,000Hp (3,000kW) Max Speed: 70Mph (113Kph)
Fuel Capacity: 5,000gal (19,000L)

The Dash 8-40CW is a 6-axle diesel-electric locomotive built by GE Transportation Systems from 1990 to 1994. It is part of the GE Dash 8 Series of freight locomotives.

This locomotive model is often referred to as a Dash 8-40CW, and is distinguished from the Dash 8-40C by the addition of a "wide" or "safety" cab. A cowl-bodied version of this locomotive, built only for the Canadian market, was the GE Dash 8-40CM.

The first Dash 8-40CW was delivered to the Union Pacific railroad in 1990. In total, GE would build 756 Dash 8-40CWs. The Dash 8-40CW was succeeded by the Dash 9-44CW in 1994.

Like most GE locomotives, the Dash 8-40CW saw continuous upgrades over the course of its production. Later model Conrail units were built with split cooling systems for the turbocharger intercooler and engine cooling (previous Dash 8 series had both on the same cooling system). The later units delivered to Conrail in 1993 and 1994 were equipped with GE's Integrated Function Displays (IFD). The IFDs are LCD displays that provide the engineer with the same information previously provided by analog gauges, as well as integrating distance counter and End of Train Device telemetry functions.

The Dash 8-40CW is powered by a 4,000-horsepower (3,000 kW) V16 7FDL diesel engine driving a GE GMG187 main alternator. The power generated by the main alternator drives 6 GE 752AG or 752AH Direct Current traction motors, each with a gear ratio of 83:20 and connected to 40-inch (1,016 mm) wheels which allow the Dash 8-40CW a maximum speed of 70mph (113Km/h).